-10 0 Printer does not support bidirectional communication through the current port
-9 0 Checking printer status...
-8 0 Viewing printer report, status unavailable
-7 0 Configuring printer settings, status unavailable
-6 0 Initial check of printer status...
-5 0 Printer busy
-4 3 Printer in unknown mode, Errcode :
-3 0 Printing...
-2 0 Printing & buffering data...
-1 5 Not accessible or offline
0 0 Online
1000 2 No new command
1001 2 Parameter Table
1002 2 Comm. sorting
1003 2 Too many slashes
1004 2 Slash w/o param
1005 2 2 same commands
1006 2 Letter incorrect
1007 2 Command incorr
1008 2 Subcomm. incorr
1009 2 Param. tab inc
1010 2 #ER x #Q !
1011 2 #ER missing
1012 2 #IM x #Q !
1013 2 Comm. flag inc
1014 2 Uninit integer
1015 2 Uninit float
1016 2 Uninit string
1017 2 Uninit discr
1018 2 Too many discr
1019 2 Uninit BCD para
1020 2 Too much image
1021 2 Uninit image par
1022 2 Too many files
1023 2 Uninit File Para
1024 2 Com. too long
1025 2 Com twice there
1026 2 Comm. w/o. flag
1027 2 Uninit parameter
1028 2 Parameter uninit
1029 2 Param. incorr
1030 2 Command incorr
1031 2 Too many slashes
1032 2 Incorrect char
1033 2 Uninit flash par
1034 2 Uninit restrict
1035 2 Uninit combi
1036 2 Wrong combi para
1037 2 Software error
1038 2 Software error
1087 2 OLV not active
1088 2 No realtimeclock
1089 2 Seek Fkt. Error
1090 2 Incomplete Job
1091 2 Wrong var field
1092 2 Rename file
1093 2 Delete file
1094 2 More than 3 figs
1097 2 Out of memory
1099 2 File end
1110 2 Opening Bracket
1111 2 Closing Bracket
1112 2 Para: No Value
1113 2 No Default Value
1114 2 < Limit value
1115 2 > Limit value
1120 2 Incorr. logo no
1121 2 Logo exists
1122 2 Creating logo
1123 2 Rename logo
1124 2 Logo file
1125 2 Delete error
1126 2 File creation
1127 2 File format
1128 2 File exists
1130 2 Float overflow
1131 2 Combi overflow
1140 2 Line too long
1141 2 Para. incorr. Bl
1150 2 Integer overflow
1160 2 String too long
1170 2 X Pos > width
1171 2 X Pos < zero
1172 2 Y Pos > length
1173 2 Y Pos < zero
1174 2 Max width: right
1175 2 Max width: left
1176 2 Max length: top
1177 2 Max length: bot
1178 2 x Dots < zero
1200 2 GetRLE reset st
1201 2 GetRLE error st
1210 2 itoa Short Strin
1240 2 New FS>E
1241 2 New Read Pointer
1242 2 New FE in job
1243 2 New delete order
1244 2 New wrong pos
1245 2 New no space
1246 2 New HP no space
1247 2 Out of memory
1260 2 TimeDate string
1270 2 #-comm. invalid
1272 2 Wrong #!
1273 2 Wrong #!C
1276 2 #!P wrong number
1277 2 Wrong #!S
1278 2 Wrong #!X
1279 2 #!X wrong number
1282 2 Spooler FB > L
1285 2 #!-comm. incorrect
1290 2 Label limit
1291 2 Draw field
1300 2 Invalid Command
1301 2 Table full
1310 2 Wrong Field ID
1320 2 No Default Value
1321 2 Bar Code Object
1322 2 Logo Object
1323 2 Line Object
1324 2 Rectangle Object
1325 2 Truedoc Object
1326 2 Fix Field Creati
1327 2 Update Field Cre
1328 2 Var Field Creati
1329 2 Count Field Crea
1330 2 Create clk. field
1331 2 Field type inv.
1332 2 Field length inc.
1333 2 Logo not there
1334 2 #YV Data incorr.
1335 2 #YV Field cont.
1336 2 #YV no. incorr.
1390 2 Web width zero
1391 2 Web > Width
1392 2 Job memory full
1393 2 Job struct creat
1394 2 Invalidation
1395 2 Label too wide
1396 2 Label too long
1397 2 Label too short
1398 2 Label too small
1470 2 X-Offset
1471 2 Y-Offset
2000 2 Double var name
2002 2 Var. data length
2003 2 Expr. bracket
2004 2 Exp. quotemark
2005 2 Exp. comma pos.
2006 2 Exp.functionname
2007 2 Exp.fct.paratype
2008 2 Exp.fct.paraCnt
2009 2 Exp. name wrong
3000 2 RS232 Overrun
3001 2 RS232 Parity
3002 2 RS232 Frame
3003 2 RS232 Overrun
3004 2 RS232 Parity
3005 2 RS232 Frame
3010 2 Spooler Overflow
3011 2 Send buffer full
4100 2 No OLV data
4101 2 OLV limit exceed
4103 2 OLV barcode type
4104 2 OLV Timeout
4105 2 No OLV response
4106 2 OLV Software
5000 2 Bus device
5001 2 No gap found
5002 2 Out of paper
5003 2 Cover open
5004 2 Rewinder mat. tear
5005 2 Knife-fault
5006 2 Head-fault
5008 2 Out of ribbon
5009 2 USI start error
5010 2 Paper jam
5012 2 Delete H8 loader
5013 2 Prog H8 loader
5014 2 Power
5015 2 Scanner
5016 2 ALX Rewinder
5017 2 Power Supply
5018 2 Dot check area
5020 2 I2C Timeout xx
5021 2 I2C Conf. xx
5022 2 I2C Busy xx
5023 2 I2C LAB xx
5024 2 I2C BER xx
5025 2 I2C Polling xx
5051 2 Barcode Infeed 1
5052 2 Barcode Infeed 2
5053 2 Barcode Infeed 3
5054 2 Barcode Infeed 4
5055 2 Infeed 1 empty
5056 2 Infeed 2 empty
5057 2 Infeed 3 empty
5058 2 Infeed 4 empty
5060 2 Stacker full
5061 2 Dispenser motor
5062 2 Disp. lift motor
5063 2 Press roll / Lever 
5064 2 Backing paper / Lever up
5100 2 No H8 response
5101 2 Headadjust error
5102 2 Dot Defective
5120 2 Home position
5121 2 Touch down
5122 2 PLC not ready
5130 2 PSU xxxxxxxx
5150 2 No USI interface
5151 2 Applic. interf
5200 2 Home position
5201 2 Touch down
5203 2 Touch down sens
5204 2 Start delay
5205 2 Applicator gen.
5206 2 Applicator resp.
5207 2 Appl. driver 1
5208 2 Appl. driver 2
5209 2 Appl. driver 3
5210 2 Appl. driver 4
5500 2 Unknown
5501 2 General
5502 2 RFID internal
5510 2 RFID COM timeout
5512 2 COM open failed
5513 2 Get baud failed
5521 2 No transponder
5522 2 Tag write err
5523 2 Tag address err
5524 2 CMD not applicable
5525 2 Tag read err
5526 2 Tag select first
5527 2 Tag RF comm err
5528 2 EEPROM failure
5529 2 Parameter range
5530 2 Unknown CMD
5531 2 Protocol length
5532 2 CMD not avail.
5540 2 ISO error #1
5541 2 ISO error #2
5542 2 ISO error #3
5543 2 ISO error #15
5544 2 ISO error #16
5545 2 ISO error #17
5546 2 ISO error #18
5547 2 ISO error #19
5548 2 ISO error #20
5549 2 ISO error ???
5550 2 Wrong tag type
5551 2 Max Tags failed
5560 2 TCS full / cover
5590 2 Odd hex string
5600 2 Job without #Q
5601 2 Job memory full
6000 2 Param. incorrect
6001 2 Nov. prog. err.
6002 2 New prog. vers
6003 2 Memory error
6004 2 Load H8 program
6005 2 Fixfont data
6006 2 Speedofont data
6010 2 Printengine soft
6030 2 Param. checksum
6031 2 New Parameters
6101 2 No sensor found
6200 2 Filesystem regis
6201 2 File sys. format
6202 2 Drive open
6203 2 Filesystem close
6204 2 Disk directory
6205 2 Write disk
6206 2 Read disk
6207 2 No file card
6300 2 Out of memory
6301 2 Incomplete job
6310 2 Centr. Timeout
6311 2 Centr. Timeout
8001 2 Shared Memory
8002 2 Stream Buffer
8103 2 TrueDoc Font
8104 2 Speedo alloc
8105 2 Load TrueType
8106 2 Fonttype wrong
8107 2 Character set
8108 2 Symbol set
8109 2 TT-specifications
8110 2 Unknown char.
8111 2 Stream type
8112 2 Font not supp.
8200 2 Fixfont number
8201 2 Font downl. full
8202 2 Font deleted
8300 2 Bar code corr
8301 2 Bar code data
8302 2 Barcode checksum
8303 2 Bar code sample
8304 2 Bar c. plain-copy
8305 2 Bar code print
8306 2 Plain-copy len
8307 2 Readline dist
8308 2 Bar code ratio
8309 2 Module range
8310 2 Bar code element
8311 2 Barcode table
8400 2 PDF417 ECC
8401 2 PDF417 Lines
8402 2 PDF417 Columns
8403 2 PDF417 Style
8404 2 PDF417 Command
8405 2 PDF417 Size
8406 2 PDF417 Details
8407 2 PDF417 Coding
8500 2 Code 25Int len
8501 2 Postcode length
8600 2 EAN Length
8601 2 UPCE Numbers sys.
8700 2 IDM Data with 0
8701 2 IDM Data length
8702 2 IDM Coding
8703 2 IDM Self-test
8704 2 IDM Init. error
8705 2 IDM rows/columns
8760 2 EAN128 field len
8761 2 EAN128 Data type
8762 2 EAN128 Ident
8800 2 Maxicode Mode
8801 2 Maxicode Sys no
8802 2 Maxicode Zipcode
8803 2 Maxicode Class
8804 2 Maxi. Sec. mess
8805 2 Maxicode Country
8830 2 Cod49 Datalength
8031 2 Cod49 wrong data
8850 2 Unknown filetype
8851 2 Graphic open
8852 2 Graphic header
8853 2 Graphic palette
8854 2 Graphic read
8856 2 Free store size
8900 2 Codablock columns
8901 2 Codablock rows
8902 2 Codablock softw
8903 2 Codablock infogr
8950 2 Logo open
8951 2 File format
8952 2 Not installed
9000 2 Wrong errornum
9001 2 Software Error
9003 2 Print head type
9005 2 No Printhead
9007 2 Bad MAC Address
9009 2 Temporary MAC
9011 2 Bootloader ext.
9013 2 Head voltage
9014 2 Motor voltage
9015 2 Network init
9016 2 DHCP Failed
9017 2 RTC read failed
9018 2 #!CA wrong Pos.
9020 2 Param. ID wrong
9022 2 No network link
9024 2 Not possible !
9030 2 Log file:CF full
9031 2 Log file: nnnn
9032 2 EP file log stop
9034 2 Use min 16MB RAM
9035 2 No printpr. stop
9036 2 DMA switch off